How to update with recovery

1,connect STB and PC via RS232

2,power on STB and press ENTER on pc immediately

3,run RS232 monitor tool on PC(putty etc.)

4,run command "store scrub 0" on pc tool(putty)

5,make burning sd-card (Kingston sd-card recommanded) with Burn\_Card\_Maker.exe(see how\_to\_make\_burning\_sd\_card.png)

6,insert burning sd-card(Kingston sd-card recommanded) to STB and reboot

7,release recovery button,STB will update with recovery image