# ANDROID BOX SETUP – REMOTE FIX

## LOCAL BOX SETUP (USB REQUIRED)

All your files are stored here: [http://pokergod.dyndns.org/Android/DMM/](http://pokergod.dyndns.org/Android/CHRIS/)

Copy UpdateScript\_DMM.sh from link above to USB key and run script via ScriptManager as always.

This will first make sure all scripts and APK files are uptodate. This will work on ANY USB key including New/Blank USB keys (No more needing me to create/update USB Keys moving forward)

Running UpdateScript\_DMM.sh will update any local box with a USB attached. Run, add to spreadsheet, wait for reboot.

## REMOTE FIX BOX (NO USB NEEDED)

Copy paste this one-liner into ScriptManager Console to initiate a full fix.

wget -O - http://50.7.232.90/Android/DMM/REMOTE\_DMM\_Setup.sh | sh

wait for box to reboot – Fixed.